PAMELA

Aborting standby mode.
Initializing main routine.
Unarchiving system files.
Loading target from config. Re-acquiring target signal.
Re-establishing PAMELA network. This may take some time...
For assistance, type /helpdoc.
>> /helpdoc
Photovisual Adaptive Mapping Encrypted-Link Actuator is used to track data flow between nodes. Can operate in single-target tracking or sector-scanning modes. Broad spectrum frequency analysis enabled. Multiple data samples required for triangulation of single signal source/destination. Visual display provides three-dimension coordinate identification (X,Y,Z), parametric signal representation (X:,Y:,Z:), and outbound signal frequency (freq).
I work well with my sister. Please use responsibly.
System Online.
Reformatting Output. One moment please.
Visuals Updated.
Launching Protocol "EndGame"...
"EndGame" Loaded.
Resolving...
"EndGame" Unloaded.
Launching Protocol "EndGame 2.0"...
"EndGame 2.0" Loaded.